<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="44.755" y1="32.248" x2="0" y2="32.248" width="0" layer="20"/>
<wire x1="0" y1="32.248" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="44.755" y2="0" width="0" layer="20"/>
<wire x1="44.755" y1="0" x2="44.755" y2="32.248" width="0" layer="20"/>
<text>AC DIMMER BOARD V1.1</text>
<text>rtwomey 2012</text>
<text>GND</text>
<text>5V</text>
<text>ZC</text>
<text>DIM</text>
<text>HOT</text>
<text>N</text>
<text>AC</text>
<text>BULB</text>
<text>HOT</text>
<text>N</text>
</plain>
<libraries>
<library name="optocoupler">
<packages>
<package name="DIL06">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="twomey">
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 220 vertical&lt;/b&gt;</description>
</package>
<package name="DIL06">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="1X2-3.5MM">
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
</packages>
</library>
<library name="con-wago-500">
<packages>
<package name="W237-102">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C050-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.4 x 4.4 mm</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="OK1" library="optocoupler" package="DIL06" value="MOC3020M">
<attribute name="MF" value="FAIRCHILD SEMICONDUCTOR"/>
<attribute name="MPN" value="MOC3020-M"/>
<attribute name="OC_FARNELL" value="1505425"/>
<attribute name="OC_NEWARK" value="72K8895"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="T1" library="twomey" package="TO220V" value="BTA12-600V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OK2" library="twomey" package="DIL06" value="H11AA11">
<attribute name="MF" value=""/>
<attribute name="MPN" value="H11A1-M"/>
<attribute name="OC_FARNELL" value="1021358"/>
<attribute name="OC_NEWARK" value="97K1793"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="rcl" package="0207/7" value="33K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="0207/7" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AC_POW" library="con-wago-500" package="W237-102" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-102"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="VALUE"/>
</element>
<element name="LIGHT" library="con-wago-500" package="W237-102" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-102"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="0207/7" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="0207/7" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="0207/7" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="0207/7" value="2.8K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C050-024X044" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP2" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP3" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP4" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="DATA" library="twomey" package="1X2-3.5MM" value=""/>
<element name="5VPOW" library="twomey" package="1X2-3.5MM" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="OK2" pad="4"/>
<contactref element="OK1" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="5VPOW" pad="1"/>
</signal>
<signal name="0V">
<contactref element="LIGHT" pad="1"/>
<contactref element="AC_POW" pad="2"/>
<contactref element="OK2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="OK2" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="+12V">
<contactref element="AC_POW" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="T1" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="R2" pad="1"/>
<contactref element="5VPOW" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="OK2" pad="5"/>
<contactref element="DATA" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="OK1" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="1"/>
<contactref element="LED1" pad="K"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="1"/>
<contactref element="LED1" pad="A"/>
<contactref element="DATA" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R5" pad="1"/>
<contactref element="OK1" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="T1" pad="1"/>
<contactref element="LIGHT" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="T1" pad="3"/>
<contactref element="OK1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
