<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<text>ASM2001</text>
<text>TinyDuino</text>
<text>RST</text>
<text>REV 4</text>
<text>GND</text>
<text>+</text>
<text>Tiny-Circuits.com</text>
<text>NOTES:</text>
<text>2.  ALL DIMENSIONS ARE GIVEN IN INCHES.</text>
<text>3.  CIRCUIT PATHS ARE FOR REFERENCE ONLY.</text>
<text>*  2 COPPER LAYERS</text>
<text>*  .024 BOARD THICKNESS</text>
<text>*  REQUIRES TOP SIDE SILKSCREEN</text>
<text>4.  HOLE SIZES SHOWN ARE FINISHED DIAMETERS AFTER PLATING.</text>
<text>5.  BOARD PLATED USING REFLOW OR SIMILAR METHOD.</text>
<text>6.  BOARD TO HAVE BLUE SOLDER MASK ON PLATED SURFACES USING WET FILM</text>
<text>SR100 OR SR1010 EPOXY. EQUIVALENT WET OR DRY FILM MAY BE USED.</text>
<text>8.  THE FOLLOWING INFORMATION APPLIES TO THIS BOARD:</text>
<text>7.  SILKSCREEN BOARD USING WHITE INK.</text>
<text>1.  PRINTED CIRCUIT BOARD MADE FROM NEMA GRADE FR-4 EPOXY LAMINATE</text>
<text>WITH 1 OUNCE COPPER PLATING AND .024 THICKNESS.</text>
<text>FABRICATION DRAWING</text>
<text>TinyDuino - 20mm</text>
<text>AS-PCB-ASM2001</text>
<text>4</text>
<wire x1="10" y1="30" x2="30" y2="30" width="0.0254" layer="20"/>
<wire x1="30" y1="30" x2="30" y2="10" width="0.0254" layer="20"/>
<wire x1="30" y1="10" x2="10" y2="10" width="0.0254" layer="20"/>
<wire x1="10" y1="10" x2="10" y2="30" width="0.0254" layer="20"/>
<hole x="11.5" y="28.5" drill="1.5"/>
<hole x="28.5" y="28.5" drill="1.5"/>
<hole x="11.5" y="11.5" drill="1.5"/>
<hole x="28.5" y="11.5" drill="1.5"/>
<wire x1="31.27" y1="31.27" x2="31.27" y2="21.73" width="2.54" layer="46"/>
<wire x1="31.27" y1="18.27" x2="31.27" y2="8.73" width="2.54" layer="46"/>
<wire x1="21.73" y1="31.27" x2="31.27" y2="31.27" width="2.54" layer="46"/>
<wire x1="8.73" y1="31.27" x2="18.27" y2="31.27" width="2.54" layer="46"/>
<wire x1="8.73" y1="21.73" x2="8.73" y2="31.27" width="2.54" layer="46"/>
<wire x1="8.73" y1="8.73" x2="8.73" y2="18.27" width="2.54" layer="46"/>
<wire x1="18.27" y1="8.73" x2="8.73" y2="8.73" width="2.54" layer="46"/>
<wire x1="31.27" y1="8.73" x2="21.73" y2="8.73" width="2.54" layer="46"/>
<text>Released under the Creative Commons Attribution Share-Alike 3.0 License</text>
<text>http://creativecommons.org/licenses/by-sa/3.0</text>
<text>Original Arduino Uno Design by Team Arduino</text>
<text>LilyPad Arduino Design by Leah Buechley and Sparkfun Electronics</text>
<text>TinyDuino, TinyLily and TinyShield Designs by TinyCircuits</text>
</plain>
<libraries>
<library name="tinycircuits">
<description>TinyCircuits Eagle Library</description>
<packages>
<package name="3013">
<description>Keystone 3013 - RETAINER COIN CELL 16MM PC T/H</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="0402">
<description>Multilayer SMD</description>
</package>
<package name="SOT-563-6">
<description>&lt;b&gt;Small Outline Transistor; 6 leads&lt;/b&gt; Reflow soldering&lt;p&gt;</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="LNJ_LED">
<description>LED GREEN SIDE VIEW SMD</description>
</package>
<package name="0603">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
<package name="APTCLGTVTR">
<description>APTCLGTVTR Tact Switch</description>
</package>
<package name="RESONATOR">
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="ATMEL_QFN32">
<description>&lt;b&gt;QFN 32&lt;/b&gt; 5 x 5 mm&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX7042.pdf</description>
</package>
<package name="DF12-32-DP">
<description>Hirose DF12 Pattern with metal fitting, 32 positions</description>
</package>
<package name="DOCFIELD-TINYCIRCUITS-PCB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="tinycircuits" package="DF12-32-DP" value="DF12-32-DP">
<attribute name="PARTNO" value="AS-ITM-00015"/>
<attribute name="VALUE" value="DF12-32-DP"/>
</element>
<element name="U1" library="tinycircuits" package="ATMEL_QFN32" value="ATMEGA328P">
<attribute name="PARTNO" value="AS-ITM-00013"/>
<attribute name="VALUE" value="ATMEGA328P-MU"/>
</element>
<element name="Y1" library="tinycircuits" package="RESONATOR" value="8MHz">
<attribute name="PARTNO" value="AS-ITM-00027"/>
<attribute name="VALUE" value="8.00MHZ"/>
</element>
<element name="R5" library="tinycircuits" package="0402" value="1M">
<attribute name="PARTNO" value="AS-ITM-00005"/>
<attribute name="VALUE" value="1.00M"/>
</element>
<element name="C4" library="tinycircuits" package="C0402" value=".1uF">
<attribute name="PARTNO" value="AS-ITM-00008"/>
<attribute name="VALUE" value="0.1uF"/>
</element>
<element name="Q1" library="tinycircuits" package="SOT-563-6" value="NTZD3152P">
<attribute name="PARTNO" value="AS-ITM-00006"/>
<attribute name="VALUE" value="NTZD3152P"/>
</element>
<element name="Q2" library="tinycircuits" package="SOT23" value="2N7002P">
<attribute name="PARTNO" value="AS-ITM-00007"/>
<attribute name="VALUE" value="2N7002P"/>
</element>
<element name="R3" library="tinycircuits" package="0402" value="100k">
<attribute name="PARTNO" value="AS-ITM-00004"/>
<attribute name="VALUE" value="100K"/>
</element>
<element name="R2" library="tinycircuits" package="0402" value="100k">
<attribute name="PARTNO" value="AS-ITM-00004"/>
<attribute name="VALUE" value="100K"/>
</element>
<element name="SW1" library="tinycircuits" package="APTCLGTVTR" value="APTCLG">
<attribute name="PARTNO" value="AS-ITM-00010"/>
<attribute name="VALUE" value="APTCLG"/>
</element>
<element name="R4" library="tinycircuits" package="0402" value="10K">
<attribute name="PARTNO" value="AS-ITM-00032"/>
<attribute name="VALUE" value="10.0K"/>
</element>
<element name="D2" library="tinycircuits" package="0603" value="CD0603">
<attribute name="PARTNO" value="AS-ITM-00009"/>
<attribute name="VALUE" value="CD0603"/>
</element>
<element name="R1" library="tinycircuits" package="0402" value="1k">
<attribute name="PARTNO" value="AS-ITM-00003"/>
<attribute name="VALUE" value="1.00K"/>
</element>
<element name="J1" library="tinycircuits" package="3013" value="3013">
<attribute name="PARTNO" value="AS-ITM-00001"/>
<attribute name="VALUE" value="3013"/>
</element>
<element name="D1" library="tinycircuits" package="LNJ_LED" value="GREEN">
<attribute name="PARTNO" value="AS-ITM-00011"/>
<attribute name="VALUE" value="GREEN"/>
</element>
<element name="C2" library="tinycircuits" package="C0603" value="10uF">
<attribute name="PARTNO" value="AS-ITM-00002"/>
<attribute name="VALUE" value="10uF"/>
</element>
<element name="C1" library="tinycircuits" package="C0603" value="10uF">
<attribute name="PARTNO" value="AS-ITM-00002"/>
<attribute name="VALUE" value="10uF"/>
</element>
<element name="C3" library="tinycircuits" package="C0402" value=".1uF">
<attribute name="PARTNO" value="AS-ITM-00008"/>
<attribute name="VALUE" value="0.1uF"/>
<attribute name="DATABASE" value="./../../../../Eagle/AkroSense-PartsDB.txt"/>
</element>
<element name="U$1" library="tinycircuits" package="DOCFIELD-TINYCIRCUITS-PCB" value="">
<attribute name="NO_BOM" value="TRUE"/>
</element>
</elements>
<signals>
<signal name="SCK">
<contactref element="U1" pad="17"/>
<contactref element="J2" pad="15"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="16"/>
<contactref element="J2" pad="17"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="15"/>
<contactref element="J2" pad="19"/>
</signal>
<signal name="SS">
<contactref element="U1" pad="14"/>
<contactref element="J2" pad="21"/>
</signal>
<signal name="IO9">
<contactref element="U1" pad="13"/>
<contactref element="J2" pad="23"/>
</signal>
<signal name="IO8">
<contactref element="U1" pad="12"/>
<contactref element="J2" pad="25"/>
</signal>
<signal name="AD5/SCL">
<contactref element="U1" pad="28"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="AD4/SDA">
<contactref element="U1" pad="27"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="AD3">
<contactref element="U1" pad="26"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="AD2">
<contactref element="U1" pad="25"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="AD1">
<contactref element="U1" pad="24"/>
<contactref element="J2" pad="9"/>
</signal>
<signal name="AD0">
<contactref element="U1" pad="23"/>
<contactref element="J2" pad="11"/>
</signal>
<signal name="IO7">
<contactref element="U1" pad="11"/>
<contactref element="J2" pad="27"/>
</signal>
<signal name="IO6">
<contactref element="U1" pad="10"/>
<contactref element="J2" pad="29"/>
</signal>
<signal name="IO5">
<contactref element="U1" pad="9"/>
<contactref element="J2" pad="31"/>
</signal>
<signal name="IO4">
<contactref element="U1" pad="2"/>
<contactref element="J2" pad="32"/>
</signal>
<signal name="IO3">
<contactref element="U1" pad="1"/>
<contactref element="J2" pad="30"/>
</signal>
<signal name="IO2">
<contactref element="U1" pad="32"/>
<contactref element="J2" pad="28"/>
</signal>
<signal name="IO1">
<contactref element="U1" pad="31"/>
<contactref element="J2" pad="26"/>
</signal>
<signal name="IO0">
<contactref element="U1" pad="30"/>
<contactref element="J2" pad="24"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="29"/>
<contactref element="SW1" pad="1"/>
<contactref element="SW1" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="J2" pad="22"/>
</signal>
<signal name="GND">
<contactref element="C4" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="EXP"/>
<contactref element="U1" pad="21"/>
<contactref element="R3" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="SW1" pad="5"/>
<contactref element="SW1" pad="2"/>
<contactref element="SW1" pad="4"/>
<contactref element="Y1" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="D1" pad="C"/>
<contactref element="J2" pad="12"/>
<contactref element="J2" pad="14"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="AREF">
<contactref element="U1" pad="20"/>
<contactref element="J2" pad="13"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="7"/>
<contactref element="Y1" pad="3"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="Y1" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="Q2" pad="3"/>
<contactref element="Q1" pad="5"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="VBATT">
<contactref element="Q1" pad="6"/>
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="4"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="Q1" pad="3"/>
<contactref element="Q1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="Q2" pad="1"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="VCC">
<contactref element="Q1" pad="1"/>
<contactref element="Q1" pad="4"/>
<contactref element="R2" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="18"/>
<contactref element="R4" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="J2" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="RSV1">
<contactref element="J2" pad="18"/>
</signal>
<signal name="RSV2">
<contactref element="J2" pad="16"/>
</signal>
<signal name="RSV0">
<contactref element="J2" pad="20"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="+3V3">
<contactref element="J2" pad="6"/>
</signal>
<signal name="VIN">
<contactref element="J2" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
