<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<text>ASD2101</text>
<text>TinyShield-USB</text>
<text>REV3</text>
<text>NOTES:</text>
<text>2.  ALL DIMENSIONS ARE GIVEN IN INCHES.</text>
<text>3.  CIRCUIT PATHS ARE FOR REFERENCE ONLY.</text>
<text>*  2 COPPER LAYERS</text>
<text>*  .024 BOARD THICKNESS</text>
<text>*  REQUIRES TOP SIDE SILKSCREEN</text>
<text>4.  HOLE SIZES SHOWN ARE FINISHED DIAMETERS AFTER PLATING.</text>
<text>5.  BOARD PLATED USING REFLOW OR SIMILAR METHOD.</text>
<text>6.  BOARD TO HAVE BLUE SOLDER MASK ON PLATED SURFACES USING WET FILM</text>
<text>SR100 OR SR1010 EPOXY. EQUIVALENT WET OR DRY FILM MAY BE USED.</text>
<text>8.  THE FOLLOWING INFORMATION APPLIES TO THIS BOARD:</text>
<text>7.  SILKSCREEN BOARD USING WHITE INK.</text>
<text>1.  PRINTED CIRCUIT BOARD MADE FROM NEMA GRADE FR-4 EPOXY LAMINATE</text>
<text>WITH 1 OUNCE COPPER PLATING AND .024 THICKNESS.</text>
<text>FABRICATION DRAWING</text>
<text>TinyShield - USB &amp; ICP</text>
<text>AS-PCB-ASD2101</text>
<text>3</text>
<text>Tiny-Circuits.com</text>
<text>ICSP</text>
<wire x1="10" y1="30" x2="30" y2="30" width="0.0254" layer="20"/>
<wire x1="30" y1="30" x2="30" y2="10" width="0.0254" layer="20"/>
<wire x1="30" y1="10" x2="10" y2="10" width="0.0254" layer="20"/>
<wire x1="10" y1="10" x2="10" y2="30" width="0.0254" layer="20"/>
<hole x="11.5" y="28.5" drill="1.5"/>
<hole x="28.5" y="28.5" drill="1.5"/>
<hole x="28.5" y="11.5" drill="1.5"/>
<hole x="11.5" y="11.5" drill="1.5"/>
<wire x1="31.27" y1="31.27" x2="31.27" y2="21.73" width="2.54" layer="46"/>
<wire x1="31.27" y1="18.27" x2="31.27" y2="8.73" width="2.54" layer="46"/>
<wire x1="31.27" y1="8.73" x2="21.73" y2="8.73" width="2.54" layer="46"/>
<wire x1="18.27" y1="8.73" x2="8.73" y2="8.73" width="2.54" layer="46"/>
<wire x1="8.73" y1="8.73" x2="8.73" y2="18.27" width="2.54" layer="46"/>
<wire x1="8.73" y1="21.73" x2="8.73" y2="31.27" width="2.54" layer="46"/>
<wire x1="8.73" y1="31.27" x2="18.27" y2="31.27" width="2.54" layer="46"/>
<wire x1="21.73" y1="31.27" x2="31.27" y2="31.27" width="2.54" layer="46"/>
<text>Released under the Creative Commons Attribution Share-Alike 3.0 License</text>
<text>http://creativecommons.org/licenses/by-sa/3.0</text>
<text>Original Arduino Uno Design by Team Arduino</text>
<text>TinyDuino, TinyLily and TinyShield Designs by TinyCircuits</text>
<text>LilyPad Arduino Design by Leah Buechley and Sparkfun Electronics</text>
</plain>
<libraries>
<library name="tinycircuits">
<description>TinyCircuits Eagle Library</description>
<packages>
<package name="MICRO_USB">
<description>Molex Micro-USB</description>
</package>
<package name="MLF32">
<description>mlf-32</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="0402">
<description>Multilayer SMD</description>
</package>
<package name="LNJ_LED">
<description>LED GREEN SIDE VIEW SMD</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="DF12-32-DS">
<description>Hirose DF12 Pattern with metal fitting, 32 positions</description>
</package>
<package name="DF12-32-DP">
<description>Hirose DF12 Pattern with metal fitting, 32 positions</description>
</package>
<package name="2X3_.05&quot;_TH_HEADER">
</package>
<package name="DOCFIELD-TINYCIRCUITS-PCB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J4" library="tinycircuits" package="DF12-32-DP" value="DF12-32-DP">
<attribute name="PARTNO" value="AS-ITM-00015"/>
<attribute name="VALUE" value="DF12-32-DP"/>
</element>
<element name="J2" library="tinycircuits" package="DF12-32-DS" value="DF12-32-DS">
<attribute name="PARTNO" value="AS-ITM-00012"/>
<attribute name="VALUE" value="DF12-32-DS"/>
</element>
<element name="J3" library="tinycircuits" package="MICRO_USB" value="47346-0001">
<attribute name="PARTNO" value="AS-ITM-00021"/>
<attribute name="VALUE" value="47346-0001"/>
</element>
<element name="U1" library="tinycircuits" package="MLF32" value="FT232RQ">
<attribute name="PARTNO" value="AS-ITM-00029"/>
</element>
<element name="C3" library="tinycircuits" package="C0603" value="10uF">
<attribute name="PARTNO" value="AS-ITM-00002"/>
<attribute name="VALUE" value="10uF"/>
</element>
<element name="C2" library="tinycircuits" package="C0402" value="0.1uF">
<attribute name="PARTNO" value="AS-ITM-00008"/>
<attribute name="VALUE" value="0.1uF"/>
</element>
<element name="C4" library="tinycircuits" package="C0402" value="0.1uF">
<attribute name="PARTNO" value="AS-ITM-00008"/>
<attribute name="VALUE" value="0.1uF"/>
</element>
<element name="C1" library="tinycircuits" package="C0402" value="0.1uF">
<attribute name="PARTNO" value="AS-ITM-00008"/>
<attribute name="VALUE" value="0.1uF"/>
</element>
<element name="R1" library="tinycircuits" package="0402" value="1.00K">
<attribute name="PARTNO" value="AS-ITM-00003"/>
<attribute name="VALUE" value="1.00K"/>
</element>
<element name="R2" library="tinycircuits" package="0402" value="1.00K">
<attribute name="PARTNO" value="AS-ITM-00003"/>
<attribute name="VALUE" value="1.00K"/>
</element>
<element name="R3" library="tinycircuits" package="0402" value="1.00K">
<attribute name="PARTNO" value="AS-ITM-00003"/>
<attribute name="VALUE" value="1.00K"/>
</element>
<element name="D1" library="tinycircuits" package="LNJ_LED" value="AMBER">
<attribute name="PARTNO" value="AS-ITM-00026"/>
<attribute name="VALUE" value="AMBER"/>
</element>
<element name="D2" library="tinycircuits" package="LNJ_LED" value="AMBER">
<attribute name="PARTNO" value="AS-ITM-00026"/>
<attribute name="VALUE" value="AMBER"/>
</element>
<element name="Q1" library="tinycircuits" package="SOT23" value="DMP2035U">
<attribute name="PARTNO" value="AS-ITM-00024"/>
<attribute name="VALUE" value="DMP2035U"/>
</element>
<element name="J1" library="tinycircuits" package="2X3_.05&quot;_TH_HEADER" value="20021111">
<attribute name="PARTNO" value="AS-ITM-00022"/>
<attribute name="VALUE" value="20021111"/>
<attribute name="DNP" value="T"/>
</element>
<element name="U$1" library="tinycircuits" package="DOCFIELD-TINYCIRCUITS-PCB" value="">
<attribute name="NO_BOM" value="TRUE"/>
</element>
</elements>
<signals>
<signal name="SCK">
<contactref element="J4" pad="15"/>
<contactref element="J2" pad="15"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="J4" pad="17"/>
<contactref element="J2" pad="17"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="J4" pad="19"/>
<contactref element="J2" pad="19"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="SS">
<contactref element="J4" pad="21"/>
<contactref element="J2" pad="21"/>
</signal>
<signal name="IO9">
<contactref element="J4" pad="23"/>
<contactref element="J2" pad="23"/>
</signal>
<signal name="IO8">
<contactref element="J4" pad="25"/>
<contactref element="J2" pad="25"/>
</signal>
<signal name="AD5/SCL">
<contactref element="J4" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="AD4/SDA">
<contactref element="J4" pad="3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="AD3">
<contactref element="J4" pad="5"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="AD2">
<contactref element="J4" pad="7"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="AD1">
<contactref element="J4" pad="9"/>
<contactref element="J2" pad="9"/>
</signal>
<signal name="AD0">
<contactref element="J4" pad="11"/>
<contactref element="J2" pad="11"/>
</signal>
<signal name="IO7">
<contactref element="J4" pad="27"/>
<contactref element="J2" pad="27"/>
</signal>
<signal name="IO6">
<contactref element="J4" pad="29"/>
<contactref element="J2" pad="29"/>
</signal>
<signal name="IO5">
<contactref element="J4" pad="31"/>
<contactref element="J2" pad="31"/>
</signal>
<signal name="GND">
<contactref element="J2" pad="12"/>
<contactref element="J2" pad="14"/>
<contactref element="J4" pad="12"/>
<contactref element="J4" pad="14"/>
<contactref element="J3" pad="P6"/>
<contactref element="J3" pad="P1"/>
<contactref element="J3" pad="P2"/>
<contactref element="J3" pad="P3"/>
<contactref element="J3" pad="P4"/>
<contactref element="J3" pad="P5"/>
<contactref element="J3" pad="5"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="24"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="17"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="33"/>
<contactref element="C4" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="J1" pad="6"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="AREF">
<contactref element="J4" pad="13"/>
<contactref element="J2" pad="13"/>
</signal>
<signal name="IO2">
<contactref element="J4" pad="28"/>
<contactref element="J2" pad="28"/>
</signal>
<signal name="IO1">
<contactref element="J4" pad="26"/>
<contactref element="J2" pad="26"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="IO0">
<contactref element="J4" pad="24"/>
<contactref element="J2" pad="24"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="RESET">
<contactref element="J4" pad="22"/>
<contactref element="J2" pad="22"/>
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="+5V">
<contactref element="Q1" pad="2"/>
<contactref element="J4" pad="8"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="RSV1">
<contactref element="J4" pad="18"/>
<contactref element="J2" pad="18"/>
</signal>
<signal name="RSV2">
<contactref element="J4" pad="16"/>
<contactref element="J2" pad="16"/>
</signal>
<signal name="RSV0">
<contactref element="J4" pad="20"/>
<contactref element="J2" pad="20"/>
</signal>
<signal name="+3V3">
<contactref element="J4" pad="6"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="VIN">
<contactref element="J4" pad="10"/>
<contactref element="J2" pad="10"/>
<contactref element="R3" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="IO3">
<contactref element="J4" pad="30"/>
<contactref element="J2" pad="30"/>
</signal>
<signal name="IO4">
<contactref element="J4" pad="32"/>
<contactref element="J2" pad="32"/>
</signal>
<signal name="N$13">
<contactref element="J3" pad="3"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="N$2">
<contactref element="J3" pad="2"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="DTR">
<contactref element="U1" pad="31"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="21"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="N$16">
<contactref element="D1" pad="C"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="N$6">
<contactref element="D1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="D2" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="USBVCC">
<contactref element="Q1" pad="3"/>
<contactref element="U1" pad="19"/>
<contactref element="J3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="VBATT">
<contactref element="J2" pad="4"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="16"/>
<contactref element="C4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
