<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="50.8" width="0.2032" layer="20"/>
<wire x1="0" y1="50.8" x2="32.131" y2="50.8" width="0.2032" layer="20"/>
<wire x1="32.131" y1="50.8" x2="32.131" y2="0" width="0.2032" layer="20"/>
<wire x1="32.131" y1="0" x2="0" y2="0" width="0.2032" layer="20"/>
<text>GND</text>
<text>VIN</text>
<text>PIN1</text>
<text>PIN2</text>
<text>PIN5</text>
<text>PIN7</text>
<text>PIN8</text>
<text>PIN9</text>
<text>CD</text>
<text>3V3</text>
<text>GND</text>
<text>USB</text>
<text>BAT</text>
<text>GND</text>
<text>VIN</text>
<text>PIN1</text>
<text>PIN2</text>
<text>PIN5</text>
<text>PIN7</text>
<text>PIN8</text>
<text>PIN9</text>
<text>CD</text>
<text>3V3</text>
<text>GND</text>
<text>imp Breakout</text>
<text>v11</text>
<text>//kentro/work/Eagle/Projects/SandBox/Jim/Electric Imp/built-for-imp16.bmp</text>
</plain>
<libraries>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SD_MMC_SOCKET">
<description>&lt;h3&gt;SD/Multi-Media Card Socket&lt;/h3&gt;
4UCONN part # 19646</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="1210">
</package>
<package name="0805">
</package>
<package name="VLF4012A">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="WSON-8-PAD">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X09_NO_SILK">
</package>
<package name="1X02_NO_SILK">
</package>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="JST-2-PTH-NS">
</package>
<package name="1X03_NO_SILK">
</package>
<package name="1X02_SMD">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SFE-NEW-WEBLOGO">
</package>
<package name="SFE-LOGO-FLAME">
</package>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MICRO-FIDUCIAL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-RF" package="SD_MMC_SOCKET" value="ELECTRIC_IMP"/>
<element name="R1" library="SparkFun-Passives" package="0402-RES" value="100k"/>
<element name="U3" library="SparkFun-DigitalIC" package="SOT23-3" value="ATSHA204-TSU"/>
<element name="C4" library="SparkFun-Passives" package="0402-CAP" value="0.1uF"/>
<element name="C2" library="SparkFun-Passives" package="0805" value="22uF"/>
<element name="L1" library="SparkFun-Passives" package="VLF4012A" value="2.2uH"/>
<element name="U2" library="SparkFun-PowerIC" package="WSON-8-PAD" value="TPS62172"/>
<element name="C1" library="SparkFun-Passives" package="1210" value="10uF"/>
<element name="JP1" library="SparkFun-Connectors" package="1X09_NO_SILK" value="M09NO_SILK"/>
<element name="JP2" library="SparkFun-Connectors" package="1X02_NO_SILK" value=""/>
<element name="R2" library="SparkFun-Passives" package="0402-RES" value="dnp"/>
<element name="X1" library="SparkFun-Connectors" package="USB-MINIB" value="USBSMD"/>
<element name="JP4" library="SparkFun-Connectors" package="JST-2-PTH-NS" value=""/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="DMG2307L-7"/>
<element name="R3" library="SparkFun-Passives" package="0402-RES" value="100k"/>
<element name="JP5" library="SparkFun-Connectors" package="1X03_NO_SILK" value=""/>
<element name="JP3" library="SparkFun-Connectors" package="1X02_SMD" value=""/>
<element name="JP6" library="SparkFun-Aesthetics" package="SFE-LOGO-FLAME" value="LOGO-SFESK"/>
<element name="JP7" library="SparkFun-Aesthetics" package="SFE-NEW-WEBLOGO" value="LOGO-SFENEW"/>
<element name="U$5" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="JP8" library="SparkFun" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="JP9" library="SparkFun" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="S1"/>
<contactref element="U1" pad="S2"/>
<contactref element="U3" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="PAD"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP1" pad="9"/>
<contactref element="U2" pad="5"/>
<contactref element="X1" pad="GND"/>
<contactref element="JP4" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="U1" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="L1" pad="P$2"/>
<contactref element="C2" pad="1"/>
<contactref element="JP1" pad="8"/>
<contactref element="R2" pad="2"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="ID">
<contactref element="U1" pad="6"/>
<contactref element="R1" pad="1"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="PIN1">
<contactref element="U1" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="PIN2">
<contactref element="U1" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="PIN5">
<contactref element="U1" pad="5"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="PIN7">
<contactref element="U1" pad="7"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="PIN8">
<contactref element="U1" pad="8"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="PIN9">
<contactref element="U1" pad="9"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="CD">
<contactref element="U1" pad="CD"/>
<contactref element="JP1" pad="7"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="7"/>
<contactref element="L1" pad="P$1"/>
</signal>
<signal name="VUSB">
<contactref element="X1" pad="VBUS"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="Q1" pad="2"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="Q1" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="VBAT">
<contactref element="JP4" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="JP3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
