<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="twomey">
<packages>
<package name="IMP002_PACKAGE">
<description>&lt;b&gt;IMP002 Solder-Down module from Electric Imp&lt;/b&gt;
&lt;br&gt;
http://devwiki.electricimp.com/lib/exe/fetch.php?media=imp002_module_20130321.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="VLF4012A">
</package>
<package name="1210">
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="WSON-8-PAD">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="JST-2-PTH-NS">
</package>
<package name="1X03_NO_SILK">
</package>
<package name="MOLEX-1X2_LOCK">
</package>
<package name="1X09">
</package>
<package name="MOLEX-1X3">
</package>
<package name="1X02_NO_SILK">
</package>
<package name="1X05">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="twomey" package="IMP002_PACKAGE" value="IMP002"/>
<element name="C2" library="SparkFun-Passives" package="0805" value="22uF"/>
<element name="L1" library="SparkFun-Passives" package="VLF4012A" value="2.2uH"/>
<element name="U2" library="SparkFun-PowerIC" package="WSON-8-PAD" value="TPS62172"/>
<element name="C1" library="SparkFun-Passives" package="1210" value="10uF"/>
<element name="X1" library="SparkFun-Connectors" package="USB-MINIB" value="USBSMD"/>
<element name="JP4" library="SparkFun-Connectors" package="JST-2-PTH-NS" value=""/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="DMG2307L-7"/>
<element name="R3" library="SparkFun-Passives" package="0402-RES" value="100k"/>
<element name="JP5" library="SparkFun-Connectors" package="1X03_NO_SILK" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="1X09" value="M09"/>
<element name="JP7" library="SparkFun-Connectors" package="MOLEX-1X2_LOCK" value="PHOTOTRANS"/>
<element name="JP8" library="SparkFun-Connectors" package="MOLEX-1X3" value="STATUS_LED"/>
<element name="JP2" library="SparkFun-Connectors" package="1X02_NO_SILK" value=""/>
<element name="R1" library="SparkFun-Resistors" package="0402-RES" value="100">
<attribute name="PROD_ID" value="RES-07863"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0402-RES" value="100">
<attribute name="PROD_ID" value="RES-07863"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0402-RES" value="100">
<attribute name="PROD_ID" value="RES-07863"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X05" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="PAD"/>
<contactref element="C1" pad="2"/>
<contactref element="U2" pad="5"/>
<contactref element="C2" pad="2"/>
<contactref element="X1" pad="GND"/>
<contactref element="JP4" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="35"/>
<contactref element="U$1" pad="32"/>
<contactref element="U$1" pad="31"/>
<contactref element="U$1" pad="30"/>
<contactref element="U$1" pad="29"/>
<contactref element="U$1" pad="28"/>
<contactref element="U$1" pad="27"/>
<contactref element="U$1" pad="26"/>
<contactref element="U$1" pad="25"/>
<contactref element="U$1" pad="24"/>
<contactref element="U$1" pad="23"/>
<contactref element="U$1" pad="17"/>
<contactref element="U$1" pad="13"/>
<contactref element="U$1" pad="7"/>
<contactref element="U$1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="L1" pad="P$2"/>
<contactref element="C2" pad="1"/>
<contactref element="U2" pad="6"/>
<contactref element="U$1" pad="18"/>
<contactref element="U$1" pad="33"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="JP5" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="7"/>
<contactref element="L1" pad="P$1"/>
</signal>
<signal name="VUSB">
<contactref element="X1" pad="VBUS"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="Q1" pad="2"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="Q1" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="VBAT">
<contactref element="JP4" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="PIN6">
<contactref element="U$1" pad="20"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="PIN7">
<contactref element="U$1" pad="21"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="PIN8">
<contactref element="U$1" pad="22"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="PIN9">
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="14"/>
</signal>
<signal name="PIN_A">
<contactref element="JP1" pad="5"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="PIN_B">
<contactref element="JP1" pad="6"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="PIN_C">
<contactref element="JP1" pad="7"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="PIN_D">
<contactref element="JP1" pad="8"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="PIN_E">
<contactref element="JP1" pad="9"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="OPTOBIAS">
<contactref element="U$1" pad="2"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="OPTOIN">
<contactref element="U$1" pad="6"/>
<contactref element="JP7" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="JP8" pad="3"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="JP8" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="RLED">
<contactref element="U$1" pad="4"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="GLED">
<contactref element="U$1" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="PIN1">
<contactref element="U$1" pad="15"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="PIN2">
<contactref element="U$1" pad="16"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="PIN5">
<contactref element="U$1" pad="19"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$5">
</signal>
</signals>
</board>
</drawing>
</eagle>
