<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<text>Advanced Lumonics, LLC</text>
<text>LED</text>
<text>BLINKUP</text>
<wire x1="59.6" y1="24.855" x2="50.2" y2="4.8" width="0.4064" layer="20" curve="-46.092845"/>
<wire x1="50.2" y1="4.8" x2="9.5" y2="4.8" width="0.4064" layer="20"/>
<wire x1="9.5" y1="4.8" x2="0" y2="26.155" width="0.4064" layer="20" curve="-43.298614"/>
<wire x1="0" y1="26.155" x2="5" y2="43" width="0.4064" layer="20" curve="-37.730488"/>
<wire x1="5" y1="43" x2="55" y2="43" width="0.4064" layer="20"/>
<wire x1="55" y1="43" x2="59.6" y2="24.855" width="0.4064" layer="20" curve="-40.377007"/>
<text>IMP-ORB
1.0 2013</text>
<text>8</text>
<text>7</text>
<text>6</text>
<text>9</text>
<text>A</text>
<text>B</text>
<text>C</text>
<text>D</text>
<text>3.3</text>
<text>GND</text>
<text>E</text>
<text>5</text>
<text>GND</text>
<text>VIN</text>
<text>1</text>
<text>2</text>
</plain>
<libraries>
<library name="twomey">
<packages>
<package name="IMP002_PACKAGE">
<description>&lt;b&gt;IMP002 Solder-Down module from Electric Imp&lt;/b&gt;
&lt;br&gt;
http://devwiki.electricimp.com/lib/exe/fetch.php?media=imp002_module_20130321.pdf</description>
</package>
<package name="APA3010SF4C">
<description>SIDE LED SMD 3.0 x 1.0 mm, three pads</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="1X09">
</package>
<package name="1X03_NO_SILK">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF-TIGHT">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="twomey" package="IMP002_PACKAGE" value="IMP002">
<attribute name="VALUE"/>
</element>
<element name="X1" library="SparkFun-Connectors" package="USB-MINIB" value="USBSMD"/>
<element name="JP1" library="SparkFun-Connectors" package="1X09" value="M09"/>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="100">
<attribute name="PROD_ID" value="RES-07866"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="100">
<attribute name="PROD_ID" value="RES-07866"/>
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="68k">
<attribute name="PROD_ID" value="RES-07866"/>
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="100k">
<attribute name="PROD_ID" value="RES-07866"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0603-CAP" value="100pF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0603-CAP" value="100pF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
</element>
<element name="U$1" library="SparkFun-Electromechanical" package="STAND-OFF-TIGHT" value=""/>
<element name="IC1" library="twomey" package="SOT223" value="REG1117">
<attribute name="OC_NEWARK" value="14P6981"/>
<attribute name="MPN" value="REG1117"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1097566"/>
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Passives" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LD1" library="twomey" package="APA3010SF4C" value=""/>
<element name="JP3" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="twomey" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
</elements>
<signals>
<signal name="GND">
<contactref element="X1" pad="GND"/>
<contactref element="U1" pad="35"/>
<contactref element="U1" pad="32"/>
<contactref element="U1" pad="31"/>
<contactref element="U1" pad="30"/>
<contactref element="U1" pad="29"/>
<contactref element="U1" pad="28"/>
<contactref element="U1" pad="27"/>
<contactref element="U1" pad="26"/>
<contactref element="U1" pad="25"/>
<contactref element="U1" pad="24"/>
<contactref element="U1" pad="23"/>
<contactref element="U1" pad="17"/>
<contactref element="U1" pad="13"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="JP4" pad="3"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="U1" pad="18"/>
<contactref element="C4" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="U1" pad="33"/>
<contactref element="U1" pad="34"/>
<contactref element="C3" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="LD1" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="PIN6">
<contactref element="U1" pad="20"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="PIN7">
<contactref element="U1" pad="21"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="PIN8">
<contactref element="U1" pad="22"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="PIN9">
<contactref element="JP1" pad="4"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="PIN_A">
<contactref element="JP1" pad="5"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="PIN_B">
<contactref element="JP1" pad="6"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="PIN_C">
<contactref element="JP1" pad="7"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="PIN_D">
<contactref element="JP1" pad="8"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="PIN_E">
<contactref element="JP1" pad="9"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="OPTOBIAS">
<contactref element="U1" pad="2"/>
<contactref element="Q1" pad="K"/>
</signal>
<signal name="OPTOIN">
<contactref element="U1" pad="6"/>
<contactref element="R4" pad="2"/>
<contactref element="Q1" pad="A"/>
</signal>
<signal name="RLED">
<contactref element="U1" pad="4"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="GLED">
<contactref element="U1" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="PIN1">
<contactref element="U1" pad="15"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="PIN2">
<contactref element="U1" pad="16"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="PIN5">
<contactref element="U1" pad="19"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="LD1" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="1"/>
<contactref element="LD1" pad="3"/>
</signal>
<signal name="VIN">
<contactref element="JP3" pad="1"/>
<contactref element="X1" pad="VBUS"/>
<contactref element="IC1" pad="3"/>
<contactref element="C1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
